Packet Tracer - Configure Initial Router Settings

NAMA : RIZKI AGUNG SENTOSA - NIM : 15200048 – KELAS : 15.3A.01

1. Topology



1. Objectives

Part 1: Verify the Default Router Configuration

Part 2: Configure and Verify the Initial Router Configuration

Part 3: Save the Running Configuration File

1. Background

In this activity, you will perform basic router configurations. You will secure access to the CLI and console port using encrypted and plain text passwords. You will also configure messages for users logging into the router. These banners also warn unauthorized users that access is prohibited. Finally, you will verify and save your running configuration.

1. Verify the Default Router Configuration
   1. Establish a console connection to R1.
      1. Choose a **Console** cable from the available connections.
      2. Click **PCA** and select **RS 232**.
      3. Click **R1** and select **Console**.
      4. Click **PCA** > **Desktop** tab > **Terminal**.
      5. Click **OK** and press **ENTER**. You are now able to configure **R1**.
   2. Enter privileged mode and examine the current configuration.

You can access all the router commands from privileged EXEC mode. However, because many of the privileged commands configure operating parameters, privileged access should be password-protected to prevent unauthorized use.

* + 1. Enter privileged EXEC mode by entering the **enable** command.

Router> **enable**

Router#

Notice that the prompt changed in the configuration to reflect privileged EXEC mode.

* + 1. Enter the **show running-config** command:

Router# **show running-config**

* + 1. Answer the following questions:

What is the router’s hostname? **Router**

How many Fast Ethernet interfaces does the Router have? **4 (interface FastEthernet0/1/3)**

How many Gigabit Ethernet interfaces does the Router have? **2** **(interface GigaEthernet0/1)**

How many Serial interfaces does the router have? 2 **(interface Serial0/0/1)**

What is the range of values shown for the vty lines? **line vty 0 4**

* + 1. Display the current contents of NVRAM.

Router# **show startup-config**

startup-config is not present

Why does the router respond with the startup-config is not present message?

**Karena tidak ada format command seperti itu, yang benar adalah copy running-config startup-config** **, atau belum diset**ting \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Configure and Verify the Initial Router Configuration

To configure parameters on a router, you may be required to move between various configuration modes. Notice how the prompt changes as you navigate through the router.

* 1. Configure the initial settings on R1.

**Note**: If you have difficulty remembering the commands, refer to the content for this topic. The commands are the same as you configured on a switch.

* + 1. **R1** as the hostname.
    2. Use the following passwords:
       1. Console: **letmein**
       2. Privileged EXEC, unencrypted: **cisco**
       3. Privileged EXEC, encrypted: **itsasecret**
    3. Encrypt all plain text passwords.
    4. Message of the day text: Unauthorized access is strictly prohibited.
  1. Verify the initial settings on R1.
     1. Verify the initial settings by viewing the configuration for R1. What command do you use?

**Copy running-config startup-config** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Exit the current console session until you see the following message:

R1 con0 is now available

Press RETURN to get started.

* + 1. Press **ENTER**; you should see the following message:

Unauthorized access is strictly prohibited.

User Access Verification

Password:

Why should every router have a message-of-the-day (MOTD) banner?

**Sebagai keterangan lebih jelas tercantum pada setiap switch, agar tidak mengubah-ubah konfigurasi kecuali orang yg memiliki hak akses**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

If you are not prompted for a password, what console line command did you forget to configure?

**Line console 0**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Enter the passwords necessary to return to privileged EXEC mode.

Why would the **enable secret** password allow access to the privileged EXEC mode and **the enable password** no longer be valid?

**Iya, kerena terdapat time out** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

If you configure any more passwords on the router, are they displayed in the configuration file as plain text or in encrypted form? Explain.

**Akan Terenkripsi semua secara otomatis**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Save the Running Configuration File
   1. Save the configuration file to NVRAM.
      1. You have configured the initial settings for **R1**. Now back up the running configuration file to NVRAM to ensure that the changes made are not lost if the system is rebooted or loses power.

What command did you enter to save the configuration to NVRAM?

**Copy running-config startup-config** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

What is the shortest, unambiguous version of this command?

Which command displays the contents of the NVRAM?

**R1#copy running-config startup-config**

**Destination filename [startup-config]?**

**Building configuration...**

**[OK]\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

* + 1. Verify that all of the parameters configured are recorded. If not, analyze the output and determine which commands were not done or were entered incorrectly. You can also click **Check Results** in the instruction window.
  1. Optional bonus: Save the startup configuration file to flash.

Although you will be learning more about managing the flash storage in a router in later chapters, you may be interested to know now that —, as an added backup procedure —, you can save your startup configuration file to flash. By default, the router still loads the startup configuration from NVRAM, but if NVRAM becomes corrupt, you can restore the startup configuration by copying it over from flash.

Complete the following steps to save the startup configuration to flash.

* + 1. Examine the contents of flash using the **show flash** command:

R1# **show flash**

How many files are currently stored in flash? **3**

Which of these files would you guess is the IOS image? **C1900-universal**

Why do you think this file is the IOS image?

**Kebanyakan file image extensionya itu adalah .bin, .iso, dan file itu sendiri yang ukururannya besar** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. Save the startup configuration file to flash using the following commands:


R1# **copy startup-config flash**

Destination filename [startup-config]

The router prompts to store the file in flash using the name in brackets. If the answer is yes, then press **ENTER**; if not, type an appropriate name and press **ENTER**.

* + 1. Use the **show flash** command to verify the startup configuration file is now stored in flash.

**Screenshot :**



1. Suggested Scoring Rubric

|  |  |  |  |
| --- | --- | --- | --- |
| Activity Section | Question Location | Possible Points | Earned Points |
| Part 1: Verify the Default Router Configuration | Step 2c | 10 |  |
| Step 2d | 2 |  |
| **Part 1 Total** | | **12** |  |
| Part 2: Configure and Verify the Initial Router Configuration | Step 2a | 2 |  |
| Step 2c | 5 |  |
| Step 2d | 6 |  |
| **Part 2 Total** | | **13** |  |
| Part 3: Save the Running Configuration File | Step 1a | 5 |  |
| Step 2a (bonus) | 5 |  |
| **Part 3 Total** | | **10** |  |
| **Packet Tracer Score** | | **80** |  |
| **Total Score (with bonus)** | | **105** |  |